# Range

## Function

This API is used to get parameter range for AI > Setup > License Plate Detection page.

> Note:

> The Range provides reference information for client UI input limits and API request limits. When sending Get and Set requests, the parameters must be strictly limited according to the Range, otherwise the request may be rejected by the device.

## Request Message

### Parameter Description

#### Table 1

Parameter | Range | Type | Description
--- | --- | --- | ---
channel | “CH1”…”CH1x” “IP_CH1”…” IP_CH1x” “WIFI_CH1”…” WIFI_CH1x” The number of channels depends on the capability of the device. | string array | Each array bit represents a channel with a string. DVR/NVR need. IPC only uses CH1
page_type | “ChannelConfig”, “AlarmConfig” | string | Data used to distinguish between the channel configuration page and the alarm configuration page

Sample:

    POST /API/AI/Setup/LPD/Range HTTP/1.1

    {
        "version": "1.0",
        "data": {"page_type": "ChannelConfig"}
    }

## Response Message

### Parameter Description

#### Table 2

Parameter | Range | Type | Description
--- | --- | --- | ---
channel_info |  | JSON object | Single Channel Information JSON show as follow Table x
page_type | “ChannelConfig”, “AarmConfig” | string | The data used to distinguish between the channel configuration page and the alarm configuration page is only needed when setting
channel_max |  | int | Maximum number of channels

#### Table x

Parameter | Range | Type | Description
--- | --- | --- | ---
CH1 |  | Json Object | JSON show as followTable 3
... |  | Json Object |
IP_CH1 |  | Json Object |
... |  | Json Object |
WIFI_CH1 |  | Json Object |
... |  | Json Object |

#### Table 3

Parameter | Range | Type | Description
--- | --- | --- | ---
status | "Offline","Online"， “Nonsupport” | string | Channel online status, only for digital channels. Note:This field does not exist when the channel is online
alarm_out | “Local->1”… ”Local->x” “IP_CH1->1”… “IP_CH1->2”… ” IP_CHx->1” ” IP_CHx->2” The number of channels depends on the capability of the device. | array | Alarm output channel Each array bit represents aalarm output channel with a string. Camera: Local->1:open，NULL:close
latch_time | "10","20","40", "60" | string | Alarm output time
record_enable | ture,false | bool | Recording channel switch
record_channel | “CH1”…”CH1x” “IP_CH1”…” IP_CH1x” “WIFI_CH1”…” | array | Alarm output channel Channel alarm linkage switch
post_recording | "0","5","10", "20","30" | string | Video delay time
send_email | true, false | bool | Outgoing mail switch
ftp_picture_upload | true, false | bool | Send mail switch Channel Capture FTP Upload switch (dedicated to NVR)
ftp_video_upload | true, false | bool | Channel video FTP upload switch (NVR special)
picture_to_cloud | true, false | bool | Image upload switch (NVR only)
video_to_cloud | true, false | bool | Video Cloud Upload Switch (NVR special)
full_screen |  | bool | FullScreen Switch (NVR only)
buzzer | "0","10","20","40", "60" | string | Buzzer time (NVR only)
show_message | true, false | bool | Display information switch
switch | true, false | bool | switch，false: close true: open
sensitivity | 0-100 | int | Detection sensitivity
snap_mode | "Default" "RealTimeMode" "IntervalMode" | string | Screenshot mode， IntervalMode JSON show as followTable 4
min_pixel | 64-1080 | int | Minimum pixel value
max_pixel | 320-1080 | int | Maximum pixel value
detection_type | "Off" "Pedestrian" "Vehicle" "Pedestrian &Vehicle" | string | Detection type, Humanoid and car shape (normal detection type)
detection_mode | "StaticMode" "MotionMode" | string | Detection mode
iva_lines | 0 not draw lines 1 draw lines | int | Preview and play back whether lines will appear
lpd_enhance |  | bool | License plate recognition enhancement
day_enhance_level | 0-255 | int | Daytime escalation
night_enhance_level | 0-255 | int | Night increase level
rule_info |  | Object | Information JSON show as followTable 5
point_num | [min:max] | array | 区域画点个数，最小3个点(min)，最大8个点(max)
detection_type | "EU_Plate" "US_Plate" | string | detection type
schedule_enable |  | bool | Schedule mode
ptz_operation_support |  | bool | (Ball machine use )supports ptz operation
light_linkage |  | bool | White light linkage alarm
enforcerlight_linkage |  | bool | Red and blue indicator linkage alarm
siren_linkage |  | bool | Alarm sound linkage alarm
http_listening |  | bool | http event push
schedule |  | Object | The schedule is shown in the tableTable 9
default_timeout | 1-120000 | int | Session timeout (range usage)

#### Table 4

Parameter | Range | Type | Description
--- | --- | --- | ---
snap_num | "1" "2" "3" "Unlimited" | string | Screenshot count
snap_frequency |  | int | Screenshot interval, unit s/pic

#### Table 5

Parameter | Range | Type | Description
--- | --- | --- | ---
rule_number1 |  | Object | Rule number 1,Information JSON show as followTable 6

#### Table 6

Parameter | Range | Type | Description
--- | --- | --- | ---
detection_range | "FullScreen" "Customize" | string | detection range
rule_rect |  | Object | rectangle,Information JSON show as followTable 7

#### Table 7

Parameter | Range | Type | Description
--- | --- | --- | ---
x1 | 0-704 | short | x1 coordinate point
y1 | 0-576 | short | y1 coordinate point
x2 | 0-704 | short | x2 coordinate point
y2 | 0-576 | short | y2 coordinate point
x3 | 0-704 | short | x3 coordinate point
y3 | 0-576 | short | y3 coordinate point
x4 | 0-704 | short | x4 coordinate point
y4 | 0-576 | short | y4 coordinate point

#### Table 8

Parameter | Range | Type | Description
--- | --- | --- | ---
cloud_video_is_used | 0~MAX_PARA_CHN_NUM | array | Id of the channel where the cloud video upload function is enabled
max_cloud_video_upload_num | MAX_CLOUD_VIDEO_RECORD_NUM | int | The maximum number of channels supported for cloud video uploading

#### Table 9

Parameter | Range | Type | Description
--- | --- | --- | ---
schedule_type | "SendEmail" "FtpPicUpload" "CloudPicUpload" "Record" "AlarmOut" "FtpVdUpload" "CloudVdUpload" "FloodLight" "Siren" "EnforcerLight" | string | Schedule type
week |  | Obejct | Weekly information is shown in the Table 10

#### Table 10

Parameter | Range | Type | Description
--- | --- | --- | ---
day | "Sun" "Mon" "Tue" "Wed" "Thu" "Fri" "Sat" | string | day
time |  | int | time

> Tips:

> The response message of the Range request may not contain all the fields in the above table, and the fields not included indicate that the device does not support this parameter configuration.

Sample:

    HTTP/1.1 200 OK
    Content-Type: application/json

    {
        "result": "success",
        "data": {
            "channel_max": 1,
            "channel_info": {
                "type": "object",
                "items": {"CH1": {
                    "type": "object",
                    "items": {
                        "status": {
                            "description": "Only offline channel has this variable.",
                            "type": "string",
                            "mode": "r",
                            "items": [
                                "Offline",
                                "Online",
                                "Nonsupport"
                            ]
                        },
                        "switch": {"type": "bool"},
                        "sensitivity": {
                            "type": "int32",
                            "mode": "r",
                            "min": 1,
                            "max": 100,
                            "default_value": 60
                        },
                        "snap_mode": {
                            "type": "string",
                            "items": [
                                "Default",
                                "RealTimeMode",
                                "IntervalMode"
                            ]
                        },
                        "snap_num": {
                            "type": "string",
                            "items": [
                                "1",
                                "2",
                                "3",
                                "Unlimited"
                            ]
                        },
                        "snap_frequency": {
                            "type": "int32",
                            "mode": "r",
                            "min": 1,
                            "max": 255,
                            "default_value": 2
                        },
                        "max_pixel": {
                            "type": "int32",
                            "mode": "r",
                            "min": 320,
                            "max": 1080,
                            "default_value": 320
                        },
                        "min_pixel": {
                            "type": "int32",
                            "mode": "r",
                            "min": 64,
                            "max": 1080,
                            "default_value": 64
                        },
                        "detection_mode": {
                            "type": "string",
                            "items": [
                                "StaticMode",
                                "MotionMode"
                            ]
                        },
                        "detection_type": {
                            "type": "string",
                            "items": [
                                "EU_Plate",
                                "US_Plate"
                            ]
                        },
                        "lpd_enhance": {"type": "bool"},
                        "day_enhance_level": {
                            "type": "int32",
                            "min": 0,
                            "max": 150
                        },
                        "night_enhance_level": {
                            "type": "int32",
                            "min": 0,
                            "max": 150
                        },
                        "rule_info": {
                            "type": "object",
                            "items": {"rule_number1": {
                                "type": "object",
                                "items": {
                                    "detection_range": {
                                        "description": "Only rule_rect has this variable.",
                                        "type": "string",
                                        "mode": "r",
                                        "items": [
                                            "FullScreen",
                                            "Customize"
                                        ]
                                    },
                                    "rule_rect": {
                                        "type": "object",
                                        "items": {
                                            "x1": {
                                                "type": "int32",
                                                "min": 0,
                                                "max": 704
                                            },
                                            "y1": {
                                                "type": "int32",
                                                "min": 0,
                                                "max": 576
                                            },
                                            "x2": {
                                                "type": "int32",
                                                "min": 0,
                                                "max": 704
                                            },
                                            "y2": {
                                                "type": "int32",
                                                "min": 0,
                                                "max": 576
                                            },
                                            "x3": {
                                                "type": "int32",
                                                "min": 0,
                                                "max": 704
                                            },
                                            "y3": {
                                                "type": "int32",
                                                "min": 0,
                                                "max": 576
                                            },
                                            "x4": {
                                                "type": "int32",
                                                "min": 0,
                                                "max": 704
                                            },
                                            "y4": {
                                                "type": "int32",
                                                "min": 0,
                                                "max": 576
                                            }
                                        }
                                    }
                                }
                            }}
                        }
                    }
                }}
            }
        }
    }

## Error Code

See Response Messages Body and Common error_code for more information.