# Get

## Function

This API is used to get Channel > POE Power page parameters.

## Request Message

None.

Sample:

    POST /API/ChannelConfig/PoePower/Get HTTP/1.1

    {
    	"version": "1.0",
    	"data": {}
    }

## Response Message

### Parameter Description

#### Table 1

Parameter | Range | Type | Description
--- | --- | --- | ---
channel | “CH1”…”CH1x” “IP_CH1”…” IP_CH1x” “WIFI_CH1”…” WIFI_CH1x” The number of channels depends on the capabilities of the device. | string array | Each array bit represents a channel with a string.

#### Table 2

Parameter | Range | Type | Description
--- | --- | --- | ---
channel_info |  | JSON Object | Channel Information JSON show as follow Table 3
actual_power |  | string | Used power
surplus_power |  | string | Surplus power
total_power |  | string | Total power
channel_min_power |  | string | Minimum power per channel.
channel_max_power |  | string | Maximum power per channel.
channel_max |  | int | Channel total

#### Table 3

Parameter | Range | Type | Description
--- | --- | --- | ---
CH1 |  | Json Object | JSON show as follow Table 4
… |  | Json Object |
IP_CH1 |  | Json Object |
… |  | Json Object |
WIFI_CH1 |  | Json Object |
… |  | Json Object |

#### Table 4

Parameter | Range | Type | Description
--- | --- | --- | ---
channel_current_power | Max length: 7byte | string | Power used by the current channel.

Sample:

    HTTP/1.1 200 OK
    Content-Type: application/json

    {
    	"result": "success",
    	"data": {
    		"channel_info": {
    			"CH1": {
    				"channel_current_power": "3.05"
    			},
    			"CH2": {
    				"channel_current_power": "2.39"
    			},
    			"CH3": {
    				"channel_current_power": "3.49"
    			},
    			"CH4": {
    				"channel_current_power": "3.61"
    			},
    			"CH5": {
    				"channel_current_power": "3.91"
    			},
    			"CH6": {
    				"channel_current_power": "3.19"
    			},
    			"CH7": {
    				"channel_current_power": "2.39"
    			},
    			"CH8": {
    				"channel_current_power": "3.94"
    			},
    			"CH9": {
    				"channel_current_power": "0.00"
    			},
    			"CH10": {
    				"channel_current_power": "2.75"
    			},
    			"CH11": {
    				"channel_current_power": "4.44"
    			},
    			"CH12": {
    				"channel_current_power": "3.55"
    			},
    			"CH13": {
    				"channel_current_power": "1.54"
    			},
    			"CH14": {
    				"channel_current_power": "2.51"
    			},
    			"CH15": {
    				"channel_current_power": "3.40"
    			},
    			"CH16": {
    				"channel_current_power": "1.92"
    			}
    		},
    		"actual_power": "46.08",
    		"surplus_power": "109.92",
    		"channel_min_power": "0",
    		"channel_max_power": "30",
    		"total_power": "156"
    	}
    }

## Error Code

See Response Messages Body and Common error_code for more information.