# Get

## Function

This API is used to get parameter for AI > Setup > Face Detection page.

## Request Message

#### Table 1

Parameter | Range | Type | Description
--- | --- | --- | ---
channel | “CH1”…”CH1x” “IP_CH1”…” IP_CH1x” “WIFI_CH1”…” WIFI_CH1x” The number of channels depends on the capabilities of the device. | string array | Each array bit represents a channel with a string. DVR/NVR need; IPC only use CH1
page_type | “ChannelConfig”, “AlarmConfig” | string | The data used to distinguish whether it is a channel configuration page or an alarm configuration page

Sample:

    POST API/AI/Setup/FD/Get HTTP/1.1

    {
        "version": "1.0",
        "data": {"page_type": "ChannelConfig"}
    }

## Response Message

## Parameter Description

#### Table 2

Parameter | Range | Type | Description
--- | --- | --- | ---
channel_info |  | JSON object | Channel Information JSON show as follow Table Table 3
page_type | “ChannelConfig” “AlarmConfig” | string | The data used to distinguish whether it is a channel configuration page or an alarm configuration page
channel_max |  | int | Maximum number of channels
agreed_to_agreement |  | bool | Whether to agree to the face protocol.
statement_file_name |  | string | The displayed face protocol file name.

#### Table 3

Parameter | Range | Type | Description
--- | --- | --- | ---
CH1 |  | Json Object | JSON show as follow Table Table 4
… |  | Json Object |
IP_CH1 |  | Json Object |
… |  | Json Object |
WIFI_CH1 |  | Json Object |
… |  | Json Object |

#### Table 4

Parameter | Range | Type | Description
--- | --- | --- | ---
status | "Offline" "Online" “Nonsupport” | string | Channel online status, only for digital channels. Note: When the channel is online, there is no such field
alarm_out | “Local->1”… ”Local->x” “IP_CH1->1”… “IP_CH1->2”… ” IP_CHx->1” ” IP_CHx->2” The number of channels depends on the capabilities of the device. | array | Alarm output channel Each array bit represents aalarm output channel with a string. Camera::Local->1:open, null value: close
latch_time | "5s","10s","20s","30s" | string | Alarm output time Ipc value 5 10 20 30
record_enable | true, false | bool | Recording channel switching
record_channel | “CH1”…”CH1x” “IP_CH1”… ” IP_CH1x” “WIFI_CH1”…” | array | Alarm output channel Channel alarm linkage switch.
post_recording | "OFF","5s","10s","20s","30s" | string | Video delay time Ipc value 0 5 10 20 30
send_email | true, false | bool | Send Email Switch
switch | true, false | bool | switch,false: close true: open
snap_mode | "RealTimeMode" "OptimalMode" "IntervalMode" | string | Screenshot mode, intervalMode JSON show as follow Table Table 5
apply_mode | "FrontalView" "MultiAngle" "Customize" | string | Customize JSON show as follow Table Table 6
min_pixel | 32-1080 | int | Minimum pixel value
max_pixel | 320-1080 | int | Maximum pixel value
face_enhance | true, false | bool | Face_enhance switch
face_attribute |  | bool | Face_attribute switch
detection_mode | "StaticMode" "MotionMode" | string | Detection mode
iva_lines | 0 Don't draw a line 1 draw a line | int | Whether there will be a line in the preview and playback
rule_info |  | Object | Information JSON show as follow Table Table 7
snap_num | "1" "2" "3" "Unlimited" | string | Number of screenshots
snap_frequency |  | int | Screenshot interval, unit s/pic
roll_range | 0-180 | int | The following default value fields are only available in Range: "default_value_frontal": frontal default value for mode "default_value_multi":multi default value for mode
pitch_range | 0-180 | int | The following default value fields are only available in Range: "default_value_frontal": frontal default value for mode "default_value_multi":multi default value for mode
yaw_range | 0-180 | int | The following default value fields are only available in Range: "default_value_frontal": frontal default value for mode "default_value_multi":multi default value for mode
picture_quality | 0-100 | int | The following default value fields are only available in Range: "default_value_frontal": frontal default value for mode "default_value_multi":multi default value for mode
schedule_enable |  | bool | Schedule mode
ptz_operation_support |  | bool | Ball machine use supports ptz operation
ftp_picture_upload |  | bool | Supports uploading pictures to ftp
picture_to_cloud |  | bool | Supports uploading pictures to cloud storage
ftp_video_upload |  | bool | Supports uploading videos to ftp
video_to_cloud |  | bool | Supports uploading videos to cloud storage
light_linkage |  | bool | White light linkage alarm
enforcerlight_linkage |  | bool | Red and blue indicator linkage alarm
siren_linkage |  | bool | Alarm sound linkage alarm
http_listening |  | bool | http event push
schedule |  | Object | The following table is displayed, as shown in the following Table 5
default_timeout | 1-120000 | int | Session timeout(range use)

#### Table 5

Parameter | Range | Type | Description
--- | --- | --- | ---
schedule_type | "SendEmail" "FtpPicUpload" "CloudPicUpload" "Record" "AlarmOut" "FtpVdUpload" "CloudVdUpload" "FloodLight" "Siren" "EnforcerLight" | string | Schedule type
week |  | Obejct | Weekly information is shown in the table Table 6

#### Table 6

Parameter | Range | Type | Description
--- | --- | --- | ---
day | "Sun" "Mon" "Tue" "Wed" "Thu" "Fri" "Sat" | string | day
time |  | int | time

#### Table 7

Parameter | Range | Type | Description
--- | --- | --- | ---
rule_number1 |  | Object | Rule number 1,information JSON show as follow Table Table 8

#### Table 8

Parameter | Range | Type | Description
--- | --- | --- | ---
rule_type | "A->B" "B->A" | string | Rule type
rule_kind | "Rect" "Line" | string | Rule type
detection_range | "FullScreen" "Customize" | string | Examination range
rule_rect |  | Object | Rectangle,information JSON show as follow Table table 9
rule_line |  | Object | Draw a line,information JSON show as follow Table table 10
point_num | [min:max] | array | The number of points drawn in the area, minimum 3 points (min), maximum 8 points (max)

#### Table 9

Parameter | Range | Type | Description
--- | --- | --- | ---
x1 | 0-704 | short | x1 Coordinate points
y1 | 0-576 | short | y1 Coordinate points
x2 | 0-704 | short | x2 Coordinate points
y2 | 0-576 | short | y2 Coordinate points
x3 | 0-704 | short | x3 Coordinate points
y3 | 0-576 | short | y3 Coordinate points
x4 | 0-704 | short | x4 Coordinate points
y4 | 0-576 | short | y4 Coordinate points
x5 | 0-704 | short | x5 Coordinate points
y5 | 0-576 | short | y5 Coordinate points
x6 | 0-704 | short | x6 Coordinate points
y6 | 0-576 | short | y6 Coordinate points
x7 | 0-704 | short | x7 Coordinate points
y7 | 0-576 | short | y7 Coordinate points
x8 | 0-704 | short | x8 Coordinate points
y8 | 0-576 | short | y8 Coordinate points

#### Table 10

Parameter | Range | Type | Description
--- | --- | --- | ---
x1 | 0-704 | short | x1 Coordinate points
y1 | 0-576 | short | y1 Coordinate points
x2 | 0-704 | short | x2 Coordinate points
y2 | 0-576 | short | y2 Coordinate points

Sample:

    HTTP/1.1 200 OK
    Content-Type: application/json

    {
        "result": "success",
        "data": {"channel_info": {"CH1": {
            "status": "Online",
            "switch": false,
            "face_attribute": false,
            "snap_mode": "OptimalMode",
            "snap_num": "1",
            "snap_frequency": 2,
            "apply_mode": "FrontalView",
            "roll_range": 30,
            "pitch_range": 30,
            "yaw_range": 45,
            "picture_quality": 100,
            "min_pixel": 64,
            "max_pixel": 640,
            "detection_mode": "StaticMode",
            "rule_info": {"rule_number1": {
                "detection_range": "FullScreen",
                "rule_kind": "Rect",
                "rule_line": {
                    "x1": 322,
                    "y1": 30,
                    "x2": 322,
                    "y2": 545
                },
                "rule_type": "A->B",
                "rule_rect": {
                    "x1": 30,
                    "y1": 30,
                    "x2": 30,
                    "y2": 545,
                    "x3": 675,
                    "y3": 545,
                    "x4": 675,
                    "y4": 30
                }
            }}
        }}}
    }

## Error Code

See Response Messages Body and Common error_code for more information.