# Set

## Function

This API is used to set Channel > Wireless Camera page parameters.

## Request Message

See Channel > Wireless Camera > Parameter Description > Table 1 for parameter description.

Sample:

    POST /API/ChannelConfig/WirelessCamera/Set HTTP/1.1

    {
    	"version": "1.0",
    	"data": {
    		"channel_info": {
    			"CH1": {
    				"channel_name": "Channel1 1111111",
    				"software_version": "V33.21.5.2_220429_50V",
    				"chn_index": "CH1",
    				"page": "chn_wireChn"
    			},
    			"CH2": {
    				"channel_name": "Channel 2",
    				"software_version": "V25.11.5.2_220407"
    			},
    			"CH3": {
    				"channel_name": "Channel 3",
    				"software_version": "V21.15.5.2_221207"
    			},
    			"CH4": {
    				"channel_name": "Channel 4",
    				"software_version": "V33.21.5.2_220520_50V"
    			},
    			"CH5": {
    				"channel_name": "Channel 5",
    				"software_version": "V33.21.5.2_220429_50V"
    			},
    			"CH6": {
    				"channel_name": "Channel 6",
    				"software_version": "V41.11.0.1_230706_W-0706"
    			}
    		},
    		"page_type": "ChannelConfig"
    	}
    }

## Response Message

Sample:

    HTTP/1.1 200 OK
    Content-Type: application/json

    {
    	"result": "success",
    	"data": {}
    }

## Error Code

See Response Messages Body and Common error_code for more information.