# Get

## Function

This API is used to get parameter for Thermal > Measurement Rule page.

## Request Message

### Parameter Description

See Thermal > Measurement Rule > Request Message >Parameter Description > Table 1 Get Parameter description.

Sample:

    POST /API/Thermal/Setup/MeasurementRules/Get HTTP/1.1

    {
        "version": "1.0",
        "data":{
            "page_type":"ChannelConfig"
            }

    }

## Response Message

### Parameter Description

see Thermal > Measurement Rule > Response Message >Parameter Description > Table 2 Get Parameter description.

Sample:

    HTTP/1.1 200 OK
    Content-Type: application/json

    {
        "result": "success",
        "data": {"channel_info": {"CH2": {
            "status": "Online",
            "id_info": [{
                "id_switch": false,
                "Id": 1,
                "rule_name": "1",
                "emissivity": 0.96,
                "target_distance": 1,
                "reflective_temp": 25,
                "alarm_temp": 40,
                "alarm_rules": "Above Max Temp",
                "duration_time": 3,
                "tolerance_temp": 3,
                "rule_info": {
                    "rule_point": {
                        "x": -1,
                        "y": -1
                    },
                    "rule_type": "Point"
                }
            }]
        }}}
    }

## Error Code

See Response message body and general error_code for more information.