# Add

## Function

This API is used to add license plate.

## Request Message

## Parameter Description

#### Table 1

Parameter | Range | Type | Description
--- | --- | --- | ---
MsgId | null |  |
PlateInfo |  | JSON array | Add License Plates JSON show as follow Table Table 2

Table 2

Parameter | Range | Type | Description
--- | --- | --- | ---
MsgId | null |  |
Id | 1-15characters | string | License plate number, unique identification.
GrpId |  | int | Group ID
PlateColor | 0-5 | int | License plate color, the possible values are as follows: enum AIPlateColor_e { APC_Blue = 0,// blue APC_Green = 1,// green APC_Yellow = 2, // yellow APC_Black = 3,// black APC_White = 4,// white APC_Other = 5,// other APC_Max };
CarBrand |  | string | Car brand
CarType |  | string | Car model
Sex |  | int | Owner gender: 0-male, 1-female
Owner | "Mike" | string | Owner name
IdCode | "415025199203050916" | string | Identification number
Job | "Software" | string | Profession
Phone | "12345678902" | string | Telephone number
Domicile | "Guangdong,Zhuhai,Xiangzhou ..." | string | Living
Remark | "Detail of this person ..." | string | Remark
EnableChnAlarm | [255, 255, 255, 255] | array | Special permission control, which controls which channels the face is allowed to be used for alarming. It is used by bit. The bit position indicates that the corresponding channel allows alarming. If this field does not exist or is empty, it means that special permission control is not used.
VoicePromptsChn | 0~255 | int | File index, when there is no audio file, this pass 255
VoicePromptsSel |  | array | Play channel, calculated by bit (bit0 is local, bit1 corresponds to front-end channel 1, bit2 corresponds to channel 2...)
VoicePromptsTm |  | array | Time period, there cannot be time conflicts among the 12 time periods

Sample:

    POST API/AI/Plates/Add HTTP/1.1

    {
        "version":"1.0",
        "data": {
            "PlateInfo": [
                {
                    "Id": "粤CW2763",
                    "GrpId": 6,
                    "PlateColor": 0,
                    "Sex": 1,
                    "CarBrand": "大众",
                    "CarType": "两厢车",
                    "Owner": "张三",
                    "IdCode": "12125180",
                    "Job": "职业",
                    "Phone": "15271859302",
                    "Domicile": "居住地1",
                    "Remark": "备注",
                    "EnableChnAlarm": []
                },
                {
                    "Id": "粤CK3961",
                    "GrpId": 6,
                    "PlateColor": 1,
                    "Sex": 1,
                    "CarBrand": "大众",
                    "CarType": "三厢车",
                    "Owner": "李四",
                    "IdCode": "12125181",
                    "Job": "职业",
                    "Phone": "15271859303",
                    "Domicile": "居住地2",
                    "Remark": "备注",
                    "EnableChnAlarm": []
                }
    		]
        }
    }

## Response Message

#### Table 3

Parameter | Range | Type | Description
--- | --- | --- | ---
MsgId | null |  |
Count |  | int | Number of groups
Result | [0, 0,…] | array | Result reference table Table 4

Table 4

Parameter | Value | Description
--- | --- | ---
AORT_SUCCESS | 0 | Success
AORT_NO_DB | -1 | No database
ORT_DB_EXEC_FAILED | -2 | Database execution failed
AORT_CALC_FEATURE_FAILED | -3 | Feature extraction failed
AORT_CANCELED | -4 | Cancelled
AORT_NO_DISK | -5 | No hard drive
AORT_DISK_ERROR | -6 | Hard disk error
AORT_EXIST | -7 | Existed
AORT_GROUP_INVALID | -8 | Group invalid
AORT_NOT_EXIST | -9 | Does not exist
AORT_MORE_FILE_EXIST | -10 | Record already exists
AORT_SEARCH_ERROR | -11 | Hard disk error
AORT_OVER_MAX_COUNT | -12 | Limit exceeded
AORT_UPDATING_FEATURE | -13 | Updating feature values
AORT_NO_USABLE_IPC | -14 | No IPC available for eigenvalue calculation
AORT_INVALID_PARAM | -15 | Invalid parameter
AORT_INVALID_FORMAT | -16 | Wrong format
AORT_INVALID_RES | -17 | Wrong resolution
AORT_INVALID_MEM | -18 | File too large error
AORT_CREAT_FAILED | -19 | Creation failed
AORT_MD5_NOT_MATCH | -20 | MD5 mismatch
AORT_POS_ERROR | -21 | Location error
AORT_SIZE_ERROR | -22 | Wrong size
AORT_NOT_READY | -23 | Not ready
AORT_INVALID_DB | -24 | Invalid database
AORT_GRP_INVALID_OR_INTERNAL | -25 | The group is invalid or the internal preset group is not allowed to be deleted
AORT_GRP_FACE_OVER_MAX | -26 | The number of faces in the roster group has exceeded the limit
AORT_NO_PERMISSION | -27 | No permission
AORT_GRP_PLATE_OVER_MAX | -28 | The number of license plates in the license plate group has exceeded the limit

Sample:

    HTTP/1.1 200 OK
    Content-Type: application/json

    {
        "data": {
            "Count": 2,
            "Result": [
                0,
                0
            ]
        }
    }

## Error Code

See Response Messages Body and Common error_code for more information.